CS:EIP = address specification (FAR address)

* This address specification will always denote THE MEMORY ADDRESS OF THE CURRENTLY EXECUTING INSTRUCTION !!!!!!

Mov cs, val

Mov eip, edx

JMP – Unconditional Jump

23 instr of CONDITIONAL Jump (the flag values)